**Main technical parameters**

|  |  |
| --- | --- |
| Type input network | Three phases 3х380V |
| Cable section: |  |
| ЖРГА.436515.001-601-604 | up to 150mm2 |
| ЖРГА.436515.001-605,606 | up to 240mm2 |
| Nominal current | up to 500А |
| Protection | IP54 |
| Earth system | TN-C, TT, IT-N,TN-S, TN-C-S |
| Fire resistance | correspond to GOST 12.1.004-91 |
| EMC | corresponded to GOST R 50656-2001 |
| Mean time between failures | 20000 hours |
| Warranty | 3 years |
| Life time expectancy | 25 years |
| Operation mode | continuously |
| Overall sizes ( H, W, D): |  |
| ЖРГА.436515.001-601,602 | 2020×865×425 |
| ЖРГА.436515.001-603,604 | 2020×1100×625 |
| ЖРГА.436515.001-701, ЖРГА.436515.001-601 | 2020×2200×625 (two cabinets) |