**Main technical parameters**

|  |  |
| --- | --- |
| Type input network | 24VDC |
| Wire section | up to 185/150mm2 |
| Nominal current | 200A |
| Protection | IP54 |
| Fire resistance | correspond to GOST 12.1.004-91 |
| [Mean time between failures](http://www.lingvo-online.ru/ru/Search/Translate/GlossaryItemExtraInfo?text=%d1%81%d1%80%d0%b5%d0%b4%d0%bd%d1%8f%d1%8f%20%d0%bd%d0%b0%d1%80%d0%b0%d0%b1%d0%be%d1%82%d0%ba%d0%b0%20%d0%bd%d0%b0%20%d0%be%d1%82%d0%ba%d0%b0%d0%b7&translation=mean%20time%20between%20failures&srcLang=ru&destLang=en) | 20000 hours |
| Warranty | 3 years |
| Life time expectancy | 25 years |
| Operating mode | continuously |
| Overall sizes (H, W, D) IBU, IFU1-IFU3 | 2312х363х425 |
| Weight | 130kg |