**Order data CPSP MI 70**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| № | Name | Input automatic breaker | Calculated capacity of MI | Capacity of USU | IT | Number order |
| 1 | CPSP MI 70 | 80А\* | up to 12kVA | 2х15kVA | 25kVA | ЖРГА.436515.001-103 |
| 2 | CPSP MI 70 | 80А\* | up to 16kVA | 2х20kVA | 30kVA | ЖРГА.436515.001-104 |
| 3 | CPSP MI 70 | 80А\* | up to 24kVA | 2х30kVA | 40kVA | ЖРГА.436515.001-105 |

\* - Nominal current of input automatic breaker could change according to project.