**Structure of IFU scheme**

FEEDER

Input power switching

Manual switching

2-stage surge protection

Control of insulation resistance

Transit of the three-phase power line

Network monitoring system

CS

RS 485

ASCPM

Remote shutdown function

Automatic current protection

Output power switching

LOAD